**ROUND TRIP TIME RTT, TIMEOUT**

EstimatedRTT = (1 - L) \* EstimatedRTT + L\*SampleRTT

TCP sender events:

1. Data received from app

2. Send packets and run timer

3. Acknowlegdement wait